=============================================================

Extraido de la pagina: <http://www.ndbc.noaa.gov/measdes.shtml\>

Detalle del significado de las medidas que recogen las boyas

Hurricane Symbol**Storm Special!** View the latest observations near [**Atlantic Tropical Depression Dolly**](http://www.ndbc.noaa.gov/radial_search.php?storm=at4).

# Measurement Descriptions and Units

Note: Station pages display the current hour's measurements in English units by default, but can be changed by the viewer to metric units. When accessing Real Time and Historical data files, the measurements are generally in metric units, as described below, and cannot be changed.

|  |  |
| --- | --- |
| STATION ID | Five-digit WMO [Station Identifier](http://www.ndbc.noaa.gov/staid.shtml) used since 1976. ID's can be reassigned to future deployments within the same 1 degree square. |
| DATE | In UTC (formerly called Greenwich Mean Time - GMT) |
| TIME | In UTC for data files/display. Station pages show current observations in station local time by default, but can be changed by the viewer to UTC. See the Acquisition Time [help topic](http://www.ndbc.noaa.gov/acq.shtml) for a more detailed description of observation times. |

Data are classified according to the following groups. Any data field that contains "9 filled" represents missing data for that observation hour. (Example: 999.0 99.0)

## Standard Meteorological Data

|  |  |
| --- | --- |
| WDIR | Wind direction (the direction the wind is coming from in degrees clockwise from true N) during the same period used for WSPD. See [Wind Averaging Methods](http://www.ndbc.noaa.gov/wndav.shtml) |
| WSPD | Wind speed (m/s) averaged over an eight-minute period for buoys and a two-minute period for land stations. Reported Hourly. See [Wind Averaging Methods](http://www.ndbc.noaa.gov/wndav.shtml). |
| GST | Peak 5 or 8 second gust speed (m/s) measured during the eight-minute or two-minute period. The 5 or 8 second period can be determined by payload, See the [Sensor Reporting, Sampling, and Accuracy](http://www.ndbc.noaa.gov/rsa.shtml) section. |
| WVHT | Significant wave height (meters) is calculated as the average of the highest one-third of all of the wave heights during the 20-minute sampling period. See the [Wave Measurements](http://www.ndbc.noaa.gov/wave.shtml) section. |
| DPD | Dominant wave period (seconds) is the period with the maximum wave energy. See the [Wave Measurements](http://www.ndbc.noaa.gov/wave.shtml) section. |
| APD | Average wave period (seconds) of all waves during the 20-minute period. See the [Wave Measurements](http://www.ndbc.noaa.gov/wave.shtml) section. |
| MWD | Mean wave direction corresponding to energy of the dominant period (DPD). The units are degrees from true North just like wind direction. See the [Wave Measurements](http://www.ndbc.noaa.gov/wave.shtml) section. |
| PRES | Sea level pressure (hPa). For C-MAN sites and Great Lakes buoys, the recorded pressure is reduced to sea level using the method described in *NWS Technical Procedures Bulletin 291* (11/14/80). |
| ATMP | Air temperature (Celsius). For sensor heights on buoys, see [Hull Descriptions](http://www.ndbc.noaa.gov/hull.shtml). For sensor heights at C-MAN stations, see [C-MAN Sensor Locations](http://www.ndbc.noaa.gov/cmanht.shtml) |
| WTMP | Sea surface temperature (Celsius). For sensor depth, see [Hull Description](http://www.ndbc.noaa.gov/hull.shtml). |
| DEWP | Dewpoint temperature taken at the same height as the air temperature measurement. |
| VIS | Station visibility (statute miles). Note that buoy stations are limited to reports from 0 to 1.9 miles. |
| PTDY | Pressure Tendency is the direction (plus or minus) and the amount of pressure change (hPa)for a three hour period ending at the time of observation. |
| TIDE | The water level in feet above or below [Mean Lower Low Water (MLLW)](http://tidesandcurrents.noaa.gov/mllw.html). |

## Derived Met Values

|  |  |
| --- | --- |
| HEAT | For more information on heat index, please see the [NWS Heat Wave](http://www.nws.noaa.gov/om/brochures/heat_wave.html) page. |
| CHILL | Please note that NDBC uses unadjusted winds to calculate wind chill. The winds are calculated at anemometer height. For more information on wind chill, please see the [NWS Wind Chill Temperature Index](http://www.nws.noaa.gov/om/windchill/index.shtml). |
| ICE | Estimated ice accretion in inches per hour based on an algorithm developed by Overland and Pease at the Pacific Marine Environmental Laboratory in the mid-1980s. The algorithm relates icing to the presently observed wind speed, air temperature, and sea surface temperature. The method is designed for trawlers in the 20 to 75 meter length range, underway at normal speeds in open seas and not heading downwind. In general, NWS forecasters translate ice accretion rates to the following categories:   * light: 0.0 to 0.24 inches of ice accretion/hour; * moderate: 0.25 to 0.8 inches/hour; and * heavy: greater than 0.8 inches/hour. |

## Supplemental Measurements Data

|  |  |
| --- | --- |
| Lowest 1 minute pressure | Lowest recorded atmospheric pressure for the hour to the nearest 0.1 hPa and the time at which it occured (hour and minute). |
| Highest 1 minute wind speed | Highest recorded wind speed for the hour to the nearest 0.1 m/s, its corresponding direction to the nearest degree, and the time at which it occured (hour and minute). |

## Continuous Winds

|  |  |
| --- | --- |
| WDIR | Ten-minute average wind direction measurements in degrees clockwise from true North. |
| WSPD | Ten-minute average wind speed values in m/s. |
| GDR | Direction, in degrees clockwise from true North, of the GSP, reported at the last hourly 10-minute segment. |
| GST | Maximum 5-second peak gust during the measurement hour, reported at the last hourly 10-minute segment. |
| GTIME | The minute of the hour that the GSP occurred, reported at the last hourly 10-minute segment. |

## Detailed Wave Summary

|  |  |
| --- | --- |
| WVHT | Significant Wave Height is the average height (meters) of the highest one-third of the waves during a 20 minute sampling period. |
| SWH | Swell height is the vertical distance (meters) between any swell crest and the succeeding swell wave trough. |
| SWP | Swell Period is the time (usually measured in seconds) that it takes successive swell wave crests or troughs pass a fixed point. |
| SWD | Swell Direction is the compass direction from which the swell wave are coming from. |
| WWH | Wind Wave Height is the vertical distance (meters) between any wind wave crest and the succeeding wind wave trough (independent of swell waves). |
| WWP | Wind Wave Period is the time (in seconds) that it takes successive wind wave crests or troughs to pass a fixed point. |
| WWD | Wind Wave Direction is the compass direction (degrees) from which the wind waves are coming. |
| Steepness | Wave steepness is the ratio of wave height to wave length and is an indicator of wave stability. When wave steepness exceeds a 1/7 ratio; the wave becomes unstable and begins to break. |
| APD | Average Wave Period is the average period (seconds) of the highest one-third of the wave observed during a 20 minute sampling period. |
| MWD | Mean wave direction corresponding to energy of the dominant period (DOMPD). The units are degrees from true North just like wind direction. See the [Wave Measurements](http://www.ndbc.noaa.gov/wave.shtml) section. |

## Spectral Wave Data

|  |  |
| --- | --- |
| Sep\_Freq | The Separation Frequency is the frequency that separates wind waves (WWH, WWP, WWD) from swell waves (SWH, SWP,SWD). NDBC inserts the value 9.999 if Sep\_Freq is missing. |
| Spectral wave density | Energy in (meter\*meter)/Hz, for each frequency bin (typically from 0.03 Hz to 0.40 Hz). |
| Spectral wave direction | Mean wave direction, in degrees from true North, for each frequency bin. A list of [directional stations](http://www.ndbc.noaa.gov/dwa.shtml) is available. |
| Directional Wave Spectrum | = C11(f) \* D(f,A), f=frequency (Hz), A=Azimuth angle measured clockwise from true North to the direction wave is from. D(f,A) = (1/PI)\*(0.5+R1\*COS(A-ALPHA1)+R2\*COS(2\*(A-ALPHA2))). R1 and R2 are the first and second normalized polar coordinates of the Fourier coefficients and are nondimensional. ALPHA1 and ALPHA2 are respectively mean and principal wave directions. In terms of Longuet-Higgins Fourier Coefficients   * R1 = (SQRT(a1\*a1+b1\*b1))/a0 * R2 = (SQRT(a2\*a2+b2\*b2))/a0 * ALPHA1 = 270.0-ARCTAN(b1,a1) * ALPHA2 = 270.0-(0.5\*ARCTAN(b2,a2)+{0. or 180.}) |
|  | Note! The R1 and R2 values in the monthly and yearly historical data files are scaled by 100, a carryover from how the data are transported to the archive centers. The units are hundredths, so the R1 and R2 values in those files should be multiplied by 0.01. |

For more information on the mathematics behind the measuring of surface water waves, see the [waves](http://www.ndbc.noaa.gov/wave.shtml) help section.

## Ocean Current Data

|  |  |
| --- | --- |
| DEP01,DEP02,... | The distance from the sea surface to the middle of the depth cells, or bins, measured in meters. |
| DIR01,DIR02,... | The direction the ocean current is flowing toward. 0-360 degrees, 360 is due north, 0 means no measurable current. |
| SPD01,SPD02,... | The speed of the ocean current measured in cm/s. |

## Ocean Current Data (Expanded ADCP format)

|  |  |
| --- | --- |
| Instrument Number | Stations may have more than one ADCP instrument. This field distinguishes these instruments by number. Valid values are 0-9, with 0 being reserved for surface measurements. |
| Bin | The bin number, ranging from 1 to 128, where 1 is the bin closest to the transducer head. |
| Depth | The distance from the sea surface to the middle of the depth cells, or bins, measured in meters. |
| Dir | The direction the ocean current is flowing toward. 0-360 degrees, 360 is due north, 0 means no measurable current. |
| Speed | The speed of the ocean current measured in cm/s. |
| ErrVl | The error velocity measured in cm/s. |
| VerVl | The vertical velocity of the ocean current measured in cm/s. |
| %Good3 | The percentage of three-beam solutions that are good. |
| %Good4 | The percentage of four-beam solutions that are good. |
| %GoodE | The percentage of transformations rejected. |
| EI1,EI2,EI3,EI4 | The echo intensity values for the four beams. Valid values are 0 to 255. EI1 = Echo Intensity for beam #1; EI2 = Echo Intensity for beam #1; EI3 = Echo Intensity for beam #3; and EI4 = Echo Intensity for beam #4. |
| CM1,CM2,CM3,CM4 | The correlation magnitude values for the four beams. Valid values are 0 to 255. CM1 = Correlation Magnitude for beam #1; CM2 = Correlation Magnitude for beam #1; CM3 = Correlation Magnitude for beam #3; and CM4 = Correlation Magnitude for beam #4. |
| Flags | The nine quality flags represent the results of the following quality tests based on their position in the flags field.  Flag 1 represents the overall bin status. Flag 2 represents the ADCP Built-In Test (BIT) status. Flag 3 represents the Error Velocity test status. Flag 4 represents the Percent Good test status. Flag 5 represents the Correlation Magnitude test status. Flag 6 represents the Vertical Velocity test status. Flag 7 represents the North Horizontal Velocity test status. Flag 8 represents the East Horizontal Velocity test status. Flag 9 represents the Echo Intensity test status.  Valid values are: 0 = quality not evaluated; 1 = failed quality test; 2 = questionable or suspect data; 3 = good data/passed quality test; and 9 = missing data. |

For more information on continuous winds and the timing of these measurements, see the [continuous winds](http://www.ndbc.noaa.gov/cwind.shtml) help section.

## Marsh-McBirney Current Measurements

|  |  |
| --- | --- |
| DIR | Direction the current is flowing TOWARDS, measured in degrees clockwise from North. |
| SPD | Current speed in cm/s. |

## Water Level

|  |  |
| --- | --- |
| TG01, TG02,...,TG10 | Six-minute water levels representing the height, in feet, of the water above or below Mean Lower Low Water (MLLW), offset by 10 ft. to prevent negative values. Please subtract 10 ft. from every value to obtain the true water level value, in reference to MLLW. |

## Oceanographic Data

|  |  |
| --- | --- |
| Depth (DEPTH) | Depth (meters) at which measurements are taken. |
| Ocean Temperature (OTMP) | The direct measurement (Celsius) of the Ocean Temperature (as opposed to the indirect measurement (see WTMP above)). |
| Conductivity (COND) | Conductivity is a measure of the electrical conductivity properties of seawater in milliSiemens per centimeter. |
| Salinity (SAL) | Salinity is computed by a known functional relationship between the measured electrical conductivity of seawater (CON), temperature (OTMP) and pressure. Salinity is computed using the Practical Salinity Scale of 1978 (PSS78) and reported in Practical Salinity Units. |
| Oxygen Concentration (O2%) | Dissolved oxygen as a percentage. |
| Oxygen Concentration (O2PPM) | Dissolved oxygen in parts per million. |
| Chlorophyll Concentration (CLCON) | Chlorophyll concentration in micrograms per liter (ug/l). |
| Turbidity (TURB) | Turbidity is an expression of the optical property that causes light to be scattered and absorbed rather than transmitted in straight lines through the sample (APHA 1980). Units are Formazine Turbidity Units (FTU). |
| pH (PH) | A measure of the acidity or alkalinity of the seawater. |
| Eh (EH) | Redox (oxidation and reduction) potential of seawater in millivolts. |

## Solar Radiation Data

|  |  |
| --- | --- |
| Shortwave Radiation  (SRAD1, SWRAD) | Average shortwave radiation in watts per square meter for the preceding hour. Sample frequency is 2 times per second (2 Hz). If present, SRAD1 is from a LI-COR LI-200 pyranometer sensor, and SWRAD is from an Eppley PSP Precision Spectral Pyranometer. |
| Longwave Radiation (LWRAD) | Average downwelling longwave radiation in watts per square meter for the preceding hour. Sample frequency is 2 times per second (2 Hz). If present, LWRAD is from an Eppley PIR Precision Infrared Radiometer. |

## DART (Tsunameters) Measurements

|  |  |
| --- | --- |
| T (TYPE) | Measurement Type:   * 1 = 15-minute measurement; * 2 = 1-minute measurement; and * 3 = 15-second measurement. |
| HEIGHT | Height of water column in meters. |
| tt = Tsunami Trigger Time, see the [Tsunami Detection Algorithm](http://www.ndbc.noaa.gov/dart/algorithm.shtml) ts = data Time Stamp(s) | |

## 24-Hour Rain Measurements

|  |  |
| --- | --- |
| 24-Hour Rain Rate | Average precipitation rate in units of millimeters per hour over 24-hour period from 00:00 to 23:59.99 GMT. |
| 24-Hour Rain Accumulation | Total accumulation of precipitation in units of millimeters on station over 24-period from 00:00 to 23:59.99 GMT. |
| Percent Time Raining in 24-Hour Period | Percentage of 144 ten-minute periods within a 24 hour period with a measurable accumulation of precipitation. |
| Flag | In the case of 24-hour rainfall measurements, a flag is assigned when over half of the 10-minute measurements from which it is derived are flagged. |

## Hourly Rain Measurements

|  |  |
| --- | --- |
| Hourly Rain Accumulation | Total accumulation of precipitation in units of millimeters on station during the 60-minute period from minute 0 to minute 59:59.99 of the hour. |
| Flag | In the case of one-hour accumulation, a flag is assigned when over half of the 10-minute measurements from which it is derived have been flagged. |

## 10-Minute Rain Measurements

|  |  |
| --- | --- |
| 10-Minute Rain Rate | Rain rate in units of millimeters per hour on station over the 10-minute period from 5 minutes before to 4 minutes 59.99 seconds after the time with which it is associated. |
| Flag | In the case of 10-minute rainfall measurements, a flag is assigned to any measurement when either the -5 or +5 minute rain measurement from which it is derived is missing or obviously an error. |

## Discontinued Measurement Abbreviations

Some historical files have column heading abbreviations that have changed over time. The old abbreviations are listed below with links to the new standardized abbreviation description.

|  |  |
| --- | --- |
| Old | New Abbreviation |
| WD | [WDIR](http://www.ndbc.noaa.gov/measdes.shtml#wdir) - Wind Direction |
| DIR | [WDIR](http://www.ndbc.noaa.gov/measdes.shtml#wdir) - 10 Minute Wind Direction |
| SPD | [WSPD](http://www.ndbc.noaa.gov/measdes.shtml#cwspd) - 10 Minute Wind Speed |
| GSP | [GST](http://www.ndbc.noaa.gov/measdes.shtml#cgst) - Gust in Continuous Winds data |
| GMN | [GTIME](http://www.ndbc.noaa.gov/measdes.shtml#gtime) - Time of Gust in Continuous Winds data |
| BARO | [PRES](http://www.ndbc.noaa.gov/measdes.shtml#pres) - Pressure |
| H0 | [WVHT](http://www.ndbc.noaa.gov/measdes.shtml#wvht) - Significant Wave Height |
| DOMPD | [DPD](http://www.ndbc.noaa.gov/measdes.shtml#dpd) - Dominant Wave Period |
| AVP | [APD](http://www.ndbc.noaa.gov/measdes.shtml#apd) - Average Wave Period |
| SRAD | [SWRAD](http://www.ndbc.noaa.gov/measdes.shtml#swrad) - Short Wave Solar Radiation |
| SRAD2 | [SWRAD](http://www.ndbc.noaa.gov/measdes.shtml#swrad) - LI-COR Short Wave Solar Radiation |
| LRAD | [LWRAD](http://www.ndbc.noaa.gov/measdes.shtml#lwrad) - Long Wave Solar Radiation |
| LRAD1 | [LWRAD](http://www.ndbc.noaa.gov/measdes.shtml#lwrad) - Long Wave Solar Radiation |